;/*++
;
;Copyright (c) 2013-2016 Intel Corporation
;
;Module Name:
;    iaLPSS2_UART2.inf
;
;Abstract:
;    INF file for installing the Intel(R) Serial IO UART Driver
;
;--*/

[Version]
Signature="$WINDOWS NT$"
Class=System
ClassGuid={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%INTEL%
DriverVer = 12/20/2021,5.123.1.1025
CatalogFile = iaLPSS2_UART2.cat

[DestinationDirs]
DefaultDestDir = 13

; ================= Class section =====================

[SourceDisksNames]
1 = %DiskId1%,,,""

[SourceDisksFiles]
iaLPSS2_UART2.sys  = 1,,

;*****************************************
; iaLPSS2_UART2 Install Section
;*****************************************

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%INTEL%=Intel,NTamd64.10.0

; For XP and later
[Intel.NTamd64.10.0]
; DisplayName               Section             DeviceId
; -----------               -------             --------
;-------------------iaLPSS2_UART2_ADL&ADP_S
%iaLPSS2_UART2.DeviceDesc0_ADL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_7A28
%iaLPSS2_UART2.DeviceDesc1_ADL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_7A29
%iaLPSS2_UART2.DeviceDesc2_ADL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_7A47
%iaLPSS2_UART2.DeviceDesc3_ADP_S%= iaLPSS2_UART2_Inst_CUSTOM, PCI\VEN_8086&DEV_7AA8
%iaLPSS2_UART2.DeviceDesc4_ADP_S%= iaLPSS2_UART2_Inst_CUSTOM, PCI\VEN_8086&DEV_7AA9
%iaLPSS2_UART2.DeviceDesc5_ADP_S%= iaLPSS2_UART2_Inst_CUSTOM, PCI\VEN_8086&DEV_7AFE
%iaLPSS2_UART2.DeviceDesc6_ADP_S%= iaLPSS2_UART2_Inst_CUSTOM, PCI\VEN_8086&DEV_7ADC

;-------------------iaLPSS2_UART2_BDW-LP
%iaLPSS2_UART2.DeviceDesc1_WPT%= iaLPSS2_UART2_Inst_SYSTEM,   ACPI\INT3434
%iaLPSS2_UART2.DeviceDesc2_WPT%= iaLPSS2_UART2_Inst_SYSTEM,   ACPI\INT3435

;-------------------iaLPSS2_UART2_BXT
%iaLPSS2_UART2.DeviceDesc1_BXT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_0ABC
%iaLPSS2_UART2.DeviceDesc2_BXT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_0ABE
%iaLPSS2_UART2.DeviceDesc3_BXT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_0AC0
%iaLPSS2_UART2.DeviceDesc4_BXT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_0AEE
%iaLPSS2_UART2.DeviceDesc5_BXT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_1ABC
%iaLPSS2_UART2.DeviceDesc6_BXT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_1ABE
%iaLPSS2_UART2.DeviceDesc7_BXT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_1AC0
%iaLPSS2_UART2.DeviceDesc8_BXT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_1AEE

;-------------------iaLPSS2_UART2_BXT_P
%iaLPSS2_UART2.DeviceDesc1_BXTP%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_5ABC
%iaLPSS2_UART2.DeviceDesc2_BXTP%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_5ABE
%iaLPSS2_UART2.DeviceDesc3_BXTP%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_5AC0
%iaLPSS2_UART2.DeviceDesc4_BXTP%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_5AEE

;-------------------iaLPSS2_UART2_CNL
%iaLPSS2_UART2.DeviceDesc1_CNL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_9DA8
%iaLPSS2_UART2.DeviceDesc2_CNL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_9DA9
%iaLPSS2_UART2.DeviceDesc3_CNL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_9DC7
%iaLPSS2_UART2.DeviceDesc11_CNL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A328
%iaLPSS2_UART2.DeviceDesc12_CNL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A329
%iaLPSS2_UART2.DeviceDesc13_CNL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A347
%iaLPSS2_UART2.DeviceDesc21_CML%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_02A8
%iaLPSS2_UART2.DeviceDesc22_CML%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_02A9
%iaLPSS2_UART2.DeviceDesc23_CML%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_02C7
%iaLPSS2_UART2.DeviceDesc31_CML%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_06A8
%iaLPSS2_UART2.DeviceDesc32_CML%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_06A9
%iaLPSS2_UART2.DeviceDesc33_CML%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_06C7

;-------------------iaLPSS2_UART2_EHL
%iaLPSS2_UART2.DeviceDesc1_EHL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_4B28
%iaLPSS2_UART2.DeviceDesc2_EHL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_4B29
%iaLPSS2_UART2.DeviceDesc3_EHL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_4B4D

;-------------------iaLPSS2_UART2_GLK
%iaLPSS2_UART2.DeviceDesc1_GLK%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_31BC
%iaLPSS2_UART2.DeviceDesc2_GLK%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_31BE
%iaLPSS2_UART2.DeviceDesc3_GLK%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_31C0
%iaLPSS2_UART2.DeviceDesc4_GLK%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_31EE

;-------------------iaLPSS2_UART2_HSW-LP
%iaLPSS2_UART2.DeviceDesc1_LPT%= iaLPSS2_UART2_Inst_SYSTEM,   ACPI\INT33C4
%iaLPSS2_UART2.DeviceDesc2_LPT%= iaLPSS2_UART2_Inst_SYSTEM,   ACPI\INT33C5

;-------------------iaLPSS2_UART2_ICL
%iaLPSS2_UART2.DeviceDesc1_ICL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_34A8
%iaLPSS2_UART2.DeviceDesc2_ICL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_34A9
%iaLPSS2_UART2.DeviceDesc3_ICL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_34C7
%iaLPSS2_UART2.DeviceDesc11_ICL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_3DA8
%iaLPSS2_UART2.DeviceDesc12_ICL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_3DA9
%iaLPSS2_UART2.DeviceDesc13_ICL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_3DAF
%iaLPSS2_UART2.DeviceDesc21_ICL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_38A8
%iaLPSS2_UART2.DeviceDesc22_ICL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_38A9
%iaLPSS2_UART2.DeviceDesc23_ICL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_38C7

;-------------------iaLPSS2_UART2_KBL
%iaLPSS2_UART2.DeviceDesc1_KBL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A2A8
%iaLPSS2_UART2.DeviceDesc2_KBL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A2A9
%iaLPSS2_UART2.DeviceDesc3_KBL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A2C7
%iaLPSS2_UART2.DeviceDesc4_KBL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_9D27
%iaLPSS2_UART2.DeviceDesc5_KBL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_9D28
%iaLPSS2_UART2.DeviceDesc6_KBL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_9D66

;-------------------iaLPSS2_UART2_LKF
%iaLPSS2_UART2.DeviceDesc1_LKF%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_98A8
%iaLPSS2_UART2.DeviceDesc2_LKF%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_98A9
%iaLPSS2_UART2.DeviceDesc3_LKF%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_98C7

;-------------------iaLPSS2_UART2_SKL
%iaLPSS2_UART2.DeviceDesc1_SPT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_9D27
%iaLPSS2_UART2.DeviceDesc2_SPT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_9D28
%iaLPSS2_UART2.DeviceDesc3_SPT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_9D66
%iaLPSS2_UART2.DeviceDesc11_SPT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A127
%iaLPSS2_UART2.DeviceDesc12_SPT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A128
%iaLPSS2_UART2.DeviceDesc13_SPT%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A166
%iaLPSS2_UART2.DeviceDesc21_KBP%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A2A7
%iaLPSS2_UART2.DeviceDesc22_KBP%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A2A8
%iaLPSS2_UART2.DeviceDesc23_KBP%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A2E6

;-------------------iaLPSS2_UART2_TGL
%iaLPSS2_UART2.DeviceDesc1_TGL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A0A8
%iaLPSS2_UART2.DeviceDesc2_TGL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A0A9
%iaLPSS2_UART2.DeviceDesc3_TGL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A0C7
%iaLPSS2_UART2.DeviceDesc11_TGL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A0DA
%iaLPSS2_UART2.DeviceDesc12_TGL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A0DB
%iaLPSS2_UART2.DeviceDesc13_TGL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A0DC
%iaLPSS2_UART2.DeviceDesc21_TGL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_A0DD
%iaLPSS2_UART2.DeviceDesc31_TGL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_43A8
%iaLPSS2_UART2.DeviceDesc32_TGL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_43A9
%iaLPSS2_UART2.DeviceDesc33_TGL%= iaLPSS2_UART2_Inst_CUSTOM,   PCI\VEN_8086&DEV_43A7

[iaLPSS2_UART2_Inst_CUSTOM.NT]
CopyFiles=Drivers_Dir
AddProperty=WDTFSOCDeviceCategory

[iaLPSS2_UART2_Inst_SYSTEM.NT]
CopyFiles=Drivers_Dir
AddProperty=WDTFSOCDeviceCategory

[WDTFSOCDeviceCategory]
{5D078032-6378-437B-8DA5-9B32B7CA3FDD},2,7,,0

[Drivers_Dir]
iaLPSS2_UART2.sys

[iaLPSS2_UART2_Inst_CUSTOM.NT.HW]
AddReg=iaLPSS2_UART2_Inst_CUSTOM.NT.HW.AddReg

[iaLPSS2_UART2_Inst_SYSTEM.NT.HW]
AddReg=iaLPSS2_UART2_Inst_SYSTEM.NT.HW.AddReg

[iaLPSS2_UART2_Inst_CUSTOM.NT.HW.AddReg]
HKR,"WDF","WdfDirectedPowerTransitionEnable",0x00010001,1

[iaLPSS2_UART2_Inst_SYSTEM.NT.HW.AddReg]
HKR,"WDF","WdfDirectedPowerTransitionEnable",0x00010001,1

;-------------- Service installation
[iaLPSS2_UART2_Inst_CUSTOM.NT.Services]
AddService = iaLPSS2_UART2,%SPSVCINST_ASSOCSERVICE%, iaLPSS2_UART2_Service_Inst_CUSTOM, iaLPSS2_UART2_EventLog_Inst_CUSTOM, System, Intel-iaLPSS2-UART2

[iaLPSS2_UART2_Inst_SYSTEM.NT.Services]
AddService = iaLPSS2_UART2_SYSTEM,%SPSVCINST_ASSOCSERVICE%, iaLPSS2_UART2_Service_Inst_SYSTEM, iaLPSS2_UART2_EventLog_Inst_SYSTEM, System, Intel-iaLPSS2-UART2

;-------------- Registry installation
[iaLPSS2_UART2_Service_Inst_CUSTOM.AddReg]
HKR,"Parameters","Framework",0x00010001,%SERCX2_FRAMEWORK%
HKR,"Parameters","ForcePIOMode",0x00010001,%PIO_MODE%
HKR,"Parameters","Platform",0x0,%PLATFORM%
HKR,"Parameters","DmaType",0x0,%CUSTOM_DMA_TYPE%

[iaLPSS2_UART2_Service_Inst_SYSTEM.AddReg]
HKR,"Parameters","Framework",0x00010001,%SERCX2_FRAMEWORK%
HKR,"Parameters","ForcePIOMode",0x00010001,%PIO_MODE%
HKR,"Parameters","Platform",0x0,%PLATFORM%
HKR,"Parameters","DmaType",0x0,%SYSTEM_DMA_TYPE%

;-------------- Registry installation
[iaLPSS2_UART2_EventLog_Inst_CUSTOM]
AddReg=iaLPSS2_UART2_EventLog_Inst_CUSTOM.AddReg, iaLPSS2_UART2_ETW.AddReg

[iaLPSS2_UART2_EventLog_Inst_SYSTEM]
AddReg=iaLPSS2_UART2_ETW.AddReg

[iaLPSS2_UART2_EventLog_Inst_CUSTOM.AddReg]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\system32\drivers\iaLPSS2_UART2.sys"
HKR,, TypesSupported,   0x00010001, 7
HKR,, ProviderGuid,     0x00000000, "{B87CAA6F-37A7-4F09-8DC4-D15572C5904E}"

[iaLPSS2_UART2_ETW.AddReg]
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-UART2/Analytic","OwningPublisher",0x0,"{B87CAA6F-37A7-4F09-8DC4-D15572C5904E}"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-UART2/Analytic","Enabled",0x00010001,0
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-UART2/Analytic","Isolation",0x00010001,1
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-UART2/Analytic","ChannelAccess",0x0,"O:BAG:SYD:(A;;0xf0007;;;SY)(A;;0x7;;;BA)(A;;0x3;;;BO)(A;;0x5;;;SO)(A;;0x1;;;IU)(A;;0x3;;;SU)(A;;0x1;;;S-1-5-3)(A;;0x2;;;S-1-5-33)(A;;0x1;;;S-1-5-32-573)"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-UART2/Analytic","Type",0x00010001,2
;HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-UART2/Analytic","Framework",0x00010001,%SERCX2_FRAMEWORK%
;HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-UART2/Analytic","ForcePIOMode",0x00010001,%PIO_MODE%
;HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-UART2/Analytic","Platform",0x0,%PLATFORM%
;HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-UART2/Analytic","DmaType",0x0,%CUSTOM_DMA_TYPE%
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{B87CAA6F-37A7-4F09-8DC4-D15572C5904E}",,0x0,"Intel-iaLPSS2-UART2"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{B87CAA6F-37A7-4F09-8DC4-D15572C5904E}","ResourceFileName",0x00020000,"%%SystemRoot%%\system32\drivers\iaLPSS2_UART2.sys"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{B87CAA6F-37A7-4F09-8DC4-D15572C5904E}","MessageFileName",0x00020000,"%%SystemRoot%%\system32\drivers\iaLPSS2_UART2.sys"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{B87CAA6F-37A7-4F09-8DC4-D15572C5904E}","Enabled",0x00010001,1
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{B87CAA6F-37A7-4F09-8DC4-D15572C5904E}\ChannelReferences\0",,0x0,"Intel-iaLPSS2-UART2/Analytic"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{B87CAA6F-37A7-4F09-8DC4-D15572C5904E}\ChannelReferences\0","Id",0x00010001,16
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{B87CAA6F-37A7-4F09-8DC4-D15572C5904E}\ChannelReferences\0","Flags",0x00010001,0
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{B87CAA6F-37A7-4F09-8DC4-D15572C5904E}\ChannelReferences","Count",0x00010001,1

; -------------- iaLPSS2_UART2 driver install sections
[iaLPSS2_UART2_Service_Inst_CUSTOM]
DisplayName    = %iaLPSS2_UART2.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START 
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %13%\iaLPSS2_UART2.sys
LoadOrderGroup = Extended Base
Dependencies   = SerCx
AddReg=iaLPSS2_UART2_Service_Inst_CUSTOM.AddReg

; -------------- iaLPSS2_UART2 driver install sections
[iaLPSS2_UART2_Service_Inst_SYSTEM]
DisplayName    = %iaLPSS2_UART2.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START 
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %13%\iaLPSS2_UART2.sys
LoadOrderGroup = Extended Base
Dependencies   = SerCx
AddReg=iaLPSS2_UART2_Service_Inst_SYSTEM.AddReg

[Strings]
SPSVCINST_ASSOCSERVICE= 0x00000002
INTEL = "Intel Corporation"
DiskId1 = "Intel(R) Serial IO Installation Disk"
;-------------------iaLPSS2_UART2_ADL&ADP_S
iaLPSS2_UART2.DeviceDesc0_ADL = "Intel(R) Serial IO UART Host Controller - 7A28"
iaLPSS2_UART2.DeviceDesc1_ADL = "Intel(R) Serial IO UART Host Controller - 7A29"
iaLPSS2_UART2.DeviceDesc2_ADL = "Intel(R) Serial IO UART Host Controller - 7A47"
iaLPSS2_UART2.DeviceDesc3_ADP_S = "Intel(R) Serial IO UART Host Controller - 7AA8"
iaLPSS2_UART2.DeviceDesc4_ADP_S = "Intel(R) Serial IO UART Host Controller - 7AA9"
iaLPSS2_UART2.DeviceDesc5_ADP_S = "Intel(R) Serial IO UART Host Controller - 7AFE"
iaLPSS2_UART2.DeviceDesc6_ADP_S = "Intel(R) Serial IO UART Host Controller - 7ADC"

;-------------------iaLPSS2_UART2_BDW-LP
iaLPSS2_UART2.DeviceDesc1_WPT = "Intel(R) Serial IO UART Host Controller - 9CE3"
iaLPSS2_UART2.DeviceDesc2_WPT = "Intel(R) Serial IO UART Host Controller - 9CE4"

;-------------------iaLPSS2_UART2_BXT
iaLPSS2_UART2.DeviceDesc1_BXT = "Intel(R) Serial IO UART Host Controller - 0ABC"
iaLPSS2_UART2.DeviceDesc2_BXT = "Intel(R) Serial IO UART Host Controller - 0ABE"
iaLPSS2_UART2.DeviceDesc3_BXT = "Intel(R) Serial IO UART Host Controller - 0AC0"
iaLPSS2_UART2.DeviceDesc4_BXT = "Intel(R) Serial IO UART Host Controller - 0AEE"
iaLPSS2_UART2.DeviceDesc5_BXT = "Intel(R) Serial IO UART Host Controller - 1ABC"
iaLPSS2_UART2.DeviceDesc6_BXT = "Intel(R) Serial IO UART Host Controller - 1ABE"
iaLPSS2_UART2.DeviceDesc7_BXT = "Intel(R) Serial IO UART Host Controller - 1AC0"
iaLPSS2_UART2.DeviceDesc8_BXT = "Intel(R) Serial IO UART Host Controller - 1AEE"

;-------------------iaLPSS2_UART2_BXT_P
iaLPSS2_UART2.DeviceDesc1_BXTP = "Intel(R) Serial IO UART Host Controller - 5ABC"
iaLPSS2_UART2.DeviceDesc2_BXTP = "Intel(R) Serial IO UART Host Controller - 5ABE"
iaLPSS2_UART2.DeviceDesc3_BXTP = "Intel(R) Serial IO UART Host Controller - 5AC0"
iaLPSS2_UART2.DeviceDesc4_BXTP = "Intel(R) Serial IO UART Host Controller - 5AEE"

;-------------------iaLPSS2_UART2_CNL
iaLPSS2_UART2.DeviceDesc1_CNL = "Intel(R) Serial IO UART Host Controller - 9DA8"
iaLPSS2_UART2.DeviceDesc2_CNL = "Intel(R) Serial IO UART Host Controller - 9DA9"
iaLPSS2_UART2.DeviceDesc3_CNL = "Intel(R) Serial IO UART Host Controller - 9DC7"
iaLPSS2_UART2.DeviceDesc11_CNL = "Intel(R) Serial IO UART Host Controller - A328"
iaLPSS2_UART2.DeviceDesc12_CNL = "Intel(R) Serial IO UART Host Controller - A329"
iaLPSS2_UART2.DeviceDesc13_CNL = "Intel(R) Serial IO UART Host Controller - A347"
iaLPSS2_UART2.DeviceDesc21_CML = "Intel(R) Serial IO UART Host Controller - 02A8"
iaLPSS2_UART2.DeviceDesc22_CML = "Intel(R) Serial IO UART Host Controller - 02A9"
iaLPSS2_UART2.DeviceDesc23_CML = "Intel(R) Serial IO UART Host Controller - 02C7"
iaLPSS2_UART2.DeviceDesc31_CML = "Intel(R) Serial IO UART Host Controller - 06A8"
iaLPSS2_UART2.DeviceDesc32_CML = "Intel(R) Serial IO UART Host Controller - 06A9"
iaLPSS2_UART2.DeviceDesc33_CML = "Intel(R) Serial IO UART Host Controller - 06C7"

;-------------------iaLPSS2_UART2_EHL
iaLPSS2_UART2.DeviceDesc1_EHL = "Intel(R) Serial IO UART Host Controller - 4B28"
iaLPSS2_UART2.DeviceDesc2_EHL = "Intel(R) Serial IO UART Host Controller - 4B29"
iaLPSS2_UART2.DeviceDesc3_EHL = "Intel(R) Serial IO UART Host Controller - 4B4D"

;-------------------iaLPSS2_UART2_GLK
iaLPSS2_UART2.DeviceDesc1_GLK = "Intel(R) Serial IO UART Host Controller - 31BC"
iaLPSS2_UART2.DeviceDesc2_GLK = "Intel(R) Serial IO UART Host Controller - 31BE"
iaLPSS2_UART2.DeviceDesc3_GLK = "Intel(R) Serial IO UART Host Controller - 31C0"
iaLPSS2_UART2.DeviceDesc4_GLK = "Intel(R) Serial IO UART Host Controller - 31EE"

;-------------------iaLPSS2_UART2_HSW-LP
iaLPSS2_UART2.DeviceDesc1_LPT = "Intel(R) Serial IO UART Host Controller - 9C63"
iaLPSS2_UART2.DeviceDesc2_LPT = "Intel(R) Serial IO UART Host Controller - 9C64"

;-------------------iaLPSS2_UART2_ICL
iaLPSS2_UART2.DeviceDesc1_ICL = "Intel(R) Serial IO UART Host Controller - 34A8"
iaLPSS2_UART2.DeviceDesc2_ICL = "Intel(R) Serial IO UART Host Controller - 34A9"
iaLPSS2_UART2.DeviceDesc3_ICL = "Intel(R) Serial IO UART Host Controller - 34C7"
iaLPSS2_UART2.DeviceDesc11_ICL = "Intel(R) Serial IO UART Host Controller - 3DA8"
iaLPSS2_UART2.DeviceDesc12_ICL = "Intel(R) Serial IO UART Host Controller - 3DA9"
iaLPSS2_UART2.DeviceDesc13_ICL = "Intel(R) Serial IO UART Host Controller - 3DAF"
iaLPSS2_UART2.DeviceDesc21_ICL = "Intel(R) Serial IO UART Host Controller - 38A8"
iaLPSS2_UART2.DeviceDesc22_ICL = "Intel(R) Serial IO UART Host Controller - 38A9"
iaLPSS2_UART2.DeviceDesc23_ICL = "Intel(R) Serial IO UART Host Controller - 38C7"

;-------------------iaLPSS2_UART2_KBL
iaLPSS2_UART2.DeviceDesc1_KBL = "Intel(R) Serial IO UART Host Controller - A2A8"
iaLPSS2_UART2.DeviceDesc2_KBL = "Intel(R) Serial IO UART Host Controller - A2A9"
iaLPSS2_UART2.DeviceDesc3_KBL = "Intel(R) Serial IO UART Host Controller - A2C7"
iaLPSS2_UART2.DeviceDesc4_KBL = "Intel(R) Serial IO UART Host Controller - 9D27"
iaLPSS2_UART2.DeviceDesc5_KBL = "Intel(R) Serial IO UART Host Controller - 9D28"
iaLPSS2_UART2.DeviceDesc6_KBL = "Intel(R) Serial IO UART Host Controller - 9D66"

;-------------------iaLPSS2_UART2_LKF
iaLPSS2_UART2.DeviceDesc1_LKF = "Intel(R) Serial IO UART Host Controller - 98A8"
iaLPSS2_UART2.DeviceDesc2_LKF = "Intel(R) Serial IO UART Host Controller - 98A9"
iaLPSS2_UART2.DeviceDesc3_LKF = "Intel(R) Serial IO UART Host Controller - 98C7"

;-------------------iaLPSS2_UART2_SKL
iaLPSS2_UART2.DeviceDesc1_SPT = "Intel(R) Serial IO UART Host Controller - 9D27"
iaLPSS2_UART2.DeviceDesc2_SPT = "Intel(R) Serial IO UART Host Controller - 9D28"
iaLPSS2_UART2.DeviceDesc3_SPT = "Intel(R) Serial IO UART Host Controller - 9D66"
iaLPSS2_UART2.DeviceDesc11_SPT = "Intel(R) Serial IO UART Host Controller - A127"
iaLPSS2_UART2.DeviceDesc12_SPT = "Intel(R) Serial IO UART Host Controller - A128"
iaLPSS2_UART2.DeviceDesc13_SPT = "Intel(R) Serial IO UART Host Controller - A166"
iaLPSS2_UART2.DeviceDesc21_KBP = "Intel(R) Serial IO UART Host Controller - A2A7"
iaLPSS2_UART2.DeviceDesc22_KBP = "Intel(R) Serial IO UART Host Controller - A2A8"
iaLPSS2_UART2.DeviceDesc23_KBP = "Intel(R) Serial IO UART Host Controller - A2E6"

;-------------------iaLPSS2_UART2_TGL
iaLPSS2_UART2.DeviceDesc1_TGL = "Intel(R) Serial IO UART Host Controller - A0A8"
iaLPSS2_UART2.DeviceDesc2_TGL = "Intel(R) Serial IO UART Host Controller - A0A9"
iaLPSS2_UART2.DeviceDesc3_TGL = "Intel(R) Serial IO UART Host Controller - A0C7"
iaLPSS2_UART2.DeviceDesc11_TGL = "Intel(R) Serial IO UART Host Controller - A0DA"
iaLPSS2_UART2.DeviceDesc12_TGL = "Intel(R) Serial IO UART Host Controller - A0DB"
iaLPSS2_UART2.DeviceDesc13_TGL = "Intel(R) Serial IO UART Host Controller - A0DC"
iaLPSS2_UART2.DeviceDesc21_TGL = "Intel(R) Serial IO UART Host Controller - A0DD"
iaLPSS2_UART2.DeviceDesc31_TGL = "Intel(R) Serial IO UART Host Controller - 43A8"
iaLPSS2_UART2.DeviceDesc32_TGL = "Intel(R) Serial IO UART Host Controller - 43A9"
iaLPSS2_UART2.DeviceDesc33_TGL = "Intel(R) Serial IO UART Host Controller - 43A7"
iaLPSS2_UART2.SVCDESC = "Intel(R) Serial IO UART Driver v2"
;
; Select sercx2 or serial.sys framework
SERCX2_FRAMEWORK=0      ; Set 1 to force sercx2 framework

; Applicable only in case serial.sys framework
PIO_MODE=0              ; Set 1 to force PIO mode
PLATFORM=LPSS2          ; LPSS2 platform
CUSTOM_DMA_TYPE=CUSTOM  ; LPSS2 platform supports Custom DMA;
SYSTEM_DMA_TYPE=SYSTEM  ; LPSS2 platform supports System DMA;
