;/*++
;
;Copyright (c) 2013-2014 Intel Corporation
;
;Module Name:
;    iaLPSS2_SPI.inf
;
;Abstract:
;    INF file for installing the Intel(R) Serial IO SPI driver
;
;--*/

[Version]
Signature="$WINDOWS NT$"
Class=System
ClassGuid={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%INTEL%
DriverVer = 12/20/2021,5.123.1.1025
CatalogFile=iaLPSS2_SPI.cat

[DestinationDirs]
DefaultDestDir = 13

; ================= Class section =====================

[SourceDisksNames]
1 = %DiskId1%,,,""

[SourceDisksFiles]
iaLPSS2_SPI.sys  = 1,,

;*****************************************
; iaLPSS2_SPI  Install Section
;*****************************************

[Manufacturer]
%INTEL%=Intel,NTamd64.10.0

[Intel.NTamd64.10.0]
;-------------------iaLPSS2_SPI_ADL & ADP_S
%iaLPSS2_SPI.DeviceDesc0_ADL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_7A2A
%iaLPSS2_SPI.DeviceDesc1_ADL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_7A2B
%iaLPSS2_SPI.DeviceDesc2_ADL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_7A7B
%iaLPSS2_SPI.DeviceDesc0_ADP_S%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_7AAA
%iaLPSS2_SPI.DeviceDesc1_ADP_S%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_7AAB
%iaLPSS2_SPI.DeviceDesc2_ADP_S%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_7AFB
%iaLPSS2_SPI.DeviceDesc3_ADP_S%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_7AF9
;-------------------iaLPSS2_SPI_BXT
%iaLPSS2_SPI.DeviceDesc0_BXT%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_0AC2
%iaLPSS2_SPI.DeviceDesc1_BXT%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_0AC4
%iaLPSS2_SPI.DeviceDesc2_BXT%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_0AC6
%iaLPSS2_SPI.DeviceDesc3_BXT%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_1AC2
%iaLPSS2_SPI.DeviceDesc4_BXT%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_1AC4
%iaLPSS2_SPI.DeviceDesc5_BXT%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_1AC6
;-------------------iaLPSS2_SPI_BXT_P
%iaLPSS2_SPI.DeviceDesc0_BXT_P%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_5AC2
%iaLPSS2_SPI.DeviceDesc1_BXT_P%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_5AC4
%iaLPSS2_SPI.DeviceDesc2_BXT_P%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_5AC6
;-------------------iaLPSS2_SPI_CNL
%iaLPSS2_SPI.DeviceDesc0_CNL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_9DAA
%iaLPSS2_SPI.DeviceDesc1_CNL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_9DAB
%iaLPSS2_SPI.DeviceDesc2_CNL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_9DFB
%iaLPSS2_SPI.DeviceDesc3_CNL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A32A
%iaLPSS2_SPI.DeviceDesc4_CNL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A32B
%iaLPSS2_SPI.DeviceDesc5_CNL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A37B
%iaLPSS2_SPI.DeviceDesc6_CNL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_02AA
%iaLPSS2_SPI.DeviceDesc7_CNL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_02AB
%iaLPSS2_SPI.DeviceDesc8_CNL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_02FB
%iaLPSS2_SPI.DeviceDesc9_CNL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_06AA
%iaLPSS2_SPI.DeviceDesc10_CNL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_06AB
%iaLPSS2_SPI.DeviceDesc11_CNL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_06FB
;-------------------iaLPSS2_SPI_EHL
%iaLPSS2_SPI.DeviceDesc0_EHL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_4B2A
%iaLPSS2_SPI.DeviceDesc1_EHL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_4B2B
%iaLPSS2_SPI.DeviceDesc2_EHL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_4B37
;-------------------iaLPSS2_SPI_GLK
%iaLPSS2_SPI.DeviceDesc0_GLK%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_31C2
%iaLPSS2_SPI.DeviceDesc1_GLK%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_31C4
%iaLPSS2_SPI.DeviceDesc2_GLK%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_31C6
;-------------------iaLPSS2_SPI_ICL
%iaLPSS2_SPI.DeviceDesc0_ICL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_34AA
%iaLPSS2_SPI.DeviceDesc1_ICL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_34AB
%iaLPSS2_SPI.DeviceDesc2_ICL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_34FB
%iaLPSS2_SPI.DeviceDesc3_ICL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_38AA
%iaLPSS2_SPI.DeviceDesc4_ICL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_38AB
%iaLPSS2_SPI.DeviceDesc5_ICL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_38FB
;-------------------iaLPSS2_SPI_LKF
%iaLPSS2_SPI.DeviceDesc0_LKF%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_98AA
%iaLPSS2_SPI.DeviceDesc1_LKF%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_98AB
%iaLPSS2_SPI.DeviceDesc2_LKF%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_98FB
;-------------------iaLPSS2_SPI_SKL
%iaLPSS2_SPI.DeviceDesc0_SKL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_9D29
%iaLPSS2_SPI.DeviceDesc1_SKL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_9D2A
%iaLPSS2_SPI.DeviceDesc2_SKL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A129
%iaLPSS2_SPI.DeviceDesc3_SKL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A12A
%iaLPSS2_SPI.DeviceDesc4_SKL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A2A9
%iaLPSS2_SPI.DeviceDesc5_SKL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A2AA
;-------------------iaLPSS2_SPI_TGL
%iaLPSS2_SPI.DeviceDesc0_TGL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A0AA
%iaLPSS2_SPI.DeviceDesc1_TGL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A0AB
%iaLPSS2_SPI.DeviceDesc2_TGL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A0FB
%iaLPSS2_SPI.DeviceDesc3_TGL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A0FD
%iaLPSS2_SPI.DeviceDesc4_TGL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A0FE
%iaLPSS2_SPI.DeviceDesc5_TGL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A0DE
%iaLPSS2_SPI.DeviceDesc6_TGL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_A0DF
%iaLPSS2_SPI.DeviceDesc7_TGL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_43AA
%iaLPSS2_SPI.DeviceDesc8_TGL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_43AB
%iaLPSS2_SPI.DeviceDesc9_TGL%=iaLPSS2_SPI_Device, PCI\VEN_8086&DEV_43FB

[iaLPSS2_SPI_Device.NT]
CopyFiles=Drivers_Dir
AddProperty=WDTFSOCDeviceCategory

[WDTFSOCDeviceCategory]
{5D078032-6378-437B-8DA5-9B32B7CA3FDD},2,7,,0

[Drivers_Dir]
iaLPSS2_SPI.sys

[iaLPSS2_SPI_Device.NT.HW]
AddReg=iaLPSS2_SPI_Device.NT.HW.AddReg

[iaLPSS2_SPI_Device.NT.HW.AddReg]
HKR,"WDF","WdfDirectedPowerTransitionEnable",0x00010001,1

;-------------- Service installation
[iaLPSS2_SPI_Device.NT.Services]
AddService = iaLPSS2_SPI,%SPSVCINST_ASSOCSERVICE%, iaLPSS2_SPI_Service_Inst, iaLPSS2_SPI_EventLog_Inst, System, Intel-iaLPSS2-SPI

;-------------- Registry installation
[iaLPSS2_SPI_EventLog_Inst]
AddReg=iaLPSS2_SPI_EventLog_Inst.AddReg, iaLPSS2_SPI_ETW.AddReg

[iaLPSS2_SPI_EventLog_Inst.AddReg]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\system32\drivers\iaLPSS2_SPI.sys"
HKR,, TypesSupported,   0x00010001, 7
HKR,, ProviderGuid,     0x00000000, "{6E112845-A8C4-4143-A631-256E8A3E7691}"

[iaLPSS2_SPI_ETW.AddReg]
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-SPI/Debug","OwningPublisher",0x0,"{6E112845-A8C4-4143-A631-256E8A3E7691}"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-SPI/Debug","Enabled",0x00010001,0
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-SPI/Debug","Isolation",0x00010001,1
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-SPI/Debug","ChannelAccess",0x0,"O:BAG:SYD:(A;;0xf0007;;;SY)(A;;0x7;;;BA)(A;;0x3;;;BO)(A;;0x5;;;SO)(A;;0x1;;;IU)(A;;0x3;;;SU)(A;;0x1;;;S-1-5-3)(A;;0x2;;;S-1-5-33)(A;;0x1;;;S-1-5-32-573)"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-SPI/Debug","Type",0x00010001,2
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-SPI/Performance","OwningPublisher",0x0,"{6E112845-A8C4-4143-A631-256E8A3E7691}"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-SPI/Performance","Enabled",0x00010001,0
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-SPI/Performance","Isolation",0x00010001,1
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-SPI/Performance","ChannelAccess",0x0,"O:BAG:SYD:(A;;0xf0007;;;SY)(A;;0x7;;;BA)(A;;0x3;;;BO)(A;;0x5;;;SO)(A;;0x1;;;IU)(A;;0x3;;;SU)(A;;0x1;;;S-1-5-3)(A;;0x2;;;S-1-5-33)(A;;0x1;;;S-1-5-32-573)"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Channels\Intel-iaLPSS2-SPI/Performance","Type",0x00010001,2
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{6E112845-A8C4-4143-A631-256E8A3E7691}",,0x0,"Intel-iaLPSS2-SPI"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{6E112845-A8C4-4143-A631-256E8A3E7691}","ResourceFileName",0x00020000,"%%SystemRoot%%\system32\drivers\iaLPSS2_SPI.sys"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{6E112845-A8C4-4143-A631-256E8A3E7691}","MessageFileName",0x00020000,"%%SystemRoot%%\system32\drivers\iaLPSS2_SPI.sys"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{6E112845-A8C4-4143-A631-256E8A3E7691}","Enabled",0x00010001,1
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{6E112845-A8C4-4143-A631-256E8A3E7691}\ChannelReferences\0",,0x0,"Intel-iaLPSS2-SPI/Debug"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{6E112845-A8C4-4143-A631-256E8A3E7691}\ChannelReferences\0","Id",0x00010001,16
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{6E112845-A8C4-4143-A631-256E8A3E7691}\ChannelReferences\0","Flags",0x00010001,0
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{6E112845-A8C4-4143-A631-256E8A3E7691}\ChannelReferences\1",,0x0,"Intel-iaLPSS2-SPI/Performance"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{6E112845-A8C4-4143-A631-256E8A3E7691}\ChannelReferences\1","Id",0x00010001,17
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{6E112845-A8C4-4143-A631-256E8A3E7691}\ChannelReferences\1","Flags",0x00010001,0
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\WINEVT\Publishers\{6E112845-A8C4-4143-A631-256E8A3E7691}\ChannelReferences","Count",0x00010001,2


; -------------- iaLPSS2_SPI driver install sections
[iaLPSS2_SPI_Service_Inst]
DisplayName    = %iaLPSS2_SPI.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START 
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %13%\iaLPSS2_SPI.sys
LoadOrderGroup = Base
Dependencies   = SpbCx

[Strings]
SPSVCINST_ASSOCSERVICE= 0x00000002
INTEL = "Intel Corporation"
DiskId1 = "Intel(R) Serial IO Installation Disk"
;-------------------iaLPSS2_SPI_ADL & ADP_S
iaLPSS2_SPI.DeviceDesc0_ADL = "Intel(R) Serial IO SPI Host Controller - 7A2A"
iaLPSS2_SPI.DeviceDesc1_ADL = "Intel(R) Serial IO SPI Host Controller - 7A2B"
iaLPSS2_SPI.DeviceDesc2_ADL = "Intel(R) Serial IO SPI Host Controller - 7A7B"
iaLPSS2_SPI.DeviceDesc0_ADP_S = "Intel(R) Serial IO SPI Host Controller - 7AAA"
iaLPSS2_SPI.DeviceDesc1_ADP_S = "Intel(R) Serial IO SPI Host Controller - 7AAB"
iaLPSS2_SPI.DeviceDesc2_ADP_S = "Intel(R) Serial IO SPI Host Controller - 7AFB"
iaLPSS2_SPI.DeviceDesc3_ADP_S = "Intel(R) Serial IO SPI Host Controller - 7AF9"
;-------------------iaLPSS2_SPI_BXT
iaLPSS2_SPI.DeviceDesc0_BXT = "Intel(R) Serial IO SPI Host Controller - 0AC2"
iaLPSS2_SPI.DeviceDesc1_BXT = "Intel(R) Serial IO SPI Host Controller - 0AC4"
iaLPSS2_SPI.DeviceDesc2_BXT = "Intel(R) Serial IO SPI Host Controller - 0AC6"
iaLPSS2_SPI.DeviceDesc3_BXT = "Intel(R) Serial IO SPI Host Controller - 1AC2"
iaLPSS2_SPI.DeviceDesc4_BXT = "Intel(R) Serial IO SPI Host Controller - 1AC4"
iaLPSS2_SPI.DeviceDesc5_BXT = "Intel(R) Serial IO SPI Host Controller - 1AC6"
;-------------------iaLPSS2_SPI_BXT_P
iaLPSS2_SPI.DeviceDesc0_BXT_P = "Intel(R) Serial IO SPI Host Controller - 5AC2"
iaLPSS2_SPI.DeviceDesc1_BXT_P = "Intel(R) Serial IO SPI Host Controller - 5AC4"
iaLPSS2_SPI.DeviceDesc2_BXT_P = "Intel(R) Serial IO SPI Host Controller - 5AC6"
;-------------------iaLPSS2_SPI_CNL
iaLPSS2_SPI.DeviceDesc0_CNL = "Intel(R) Serial IO SPI Host Controller - 9DAA"
iaLPSS2_SPI.DeviceDesc1_CNL = "Intel(R) Serial IO SPI Host Controller - 9DAB"
iaLPSS2_SPI.DeviceDesc2_CNL = "Intel(R) Serial IO SPI Host Controller - 9DFB"
iaLPSS2_SPI.DeviceDesc3_CNL = "Intel(R) Serial IO SPI Host Controller - A32A"
iaLPSS2_SPI.DeviceDesc4_CNL = "Intel(R) Serial IO SPI Host Controller - A32B"
iaLPSS2_SPI.DeviceDesc5_CNL = "Intel(R) Serial IO SPI Host Controller - A37B"
iaLPSS2_SPI.DeviceDesc6_CNL = "Intel(R) Serial IO SPI Host Controller - 02AA"
iaLPSS2_SPI.DeviceDesc7_CNL = "Intel(R) Serial IO SPI Host Controller - 02AB"
iaLPSS2_SPI.DeviceDesc8_CNL = "Intel(R) Serial IO SPI Host Controller - 02FB"
iaLPSS2_SPI.DeviceDesc9_CNL = "Intel(R) Serial IO SPI Host Controller - 06AA"
iaLPSS2_SPI.DeviceDesc10_CNL = "Intel(R) Serial IO SPI Host Controller - 06AB"
iaLPSS2_SPI.DeviceDesc11_CNL = "Intel(R) Serial IO SPI Host Controller - 06FB"
;-------------------iaLPSS2_SPI_EHL
iaLPSS2_SPI.DeviceDesc0_EHL = "Intel(R) Serial IO SPI Host Controller - 4B2A"
iaLPSS2_SPI.DeviceDesc1_EHL = "Intel(R) Serial IO SPI Host Controller - 4B2B"
iaLPSS2_SPI.DeviceDesc2_EHL = "Intel(R) Serial IO SPI Host Controller - 4B37"
;-------------------iaLPSS2_SPI_GLK
iaLPSS2_SPI.DeviceDesc0_GLK = "Intel(R) Serial IO SPI Host Controller - 31C2"
iaLPSS2_SPI.DeviceDesc1_GLK = "Intel(R) Serial IO SPI Host Controller - 31C4"
iaLPSS2_SPI.DeviceDesc2_GLK = "Intel(R) Serial IO SPI Host Controller - 31C6"
;-------------------iaLPSS2_SPI_ICL
iaLPSS2_SPI.DeviceDesc0_ICL = "Intel(R) Serial IO SPI Host Controller - 34AA"
iaLPSS2_SPI.DeviceDesc1_ICL = "Intel(R) Serial IO SPI Host Controller - 34AB"
iaLPSS2_SPI.DeviceDesc2_ICL = "Intel(R) Serial IO SPI Host Controller - 34FB"
iaLPSS2_SPI.DeviceDesc3_ICL = "Intel(R) Serial IO SPI Host Controller - 38AA"
iaLPSS2_SPI.DeviceDesc4_ICL = "Intel(R) Serial IO SPI Host Controller - 38AB"
iaLPSS2_SPI.DeviceDesc5_ICL = "Intel(R) Serial IO SPI Host Controller - 38FB"
;-------------------iaLPSS2_SPI_LKF
iaLPSS2_SPI.DeviceDesc0_LKF = "Intel(R) Serial IO SPI Host Controller - 98AA"
iaLPSS2_SPI.DeviceDesc1_LKF = "Intel(R) Serial IO SPI Host Controller - 98AB"
iaLPSS2_SPI.DeviceDesc2_LKF = "Intel(R) Serial IO SPI Host Controller - 98FB"
;-------------------iaLPSS2_SPI_SKL
iaLPSS2_SPI.DeviceDesc0_SKL = "Intel(R) Serial IO SPI Host Controller - 9D29"
iaLPSS2_SPI.DeviceDesc1_SKL = "Intel(R) Serial IO SPI Host Controller - 9D2A"
iaLPSS2_SPI.DeviceDesc2_SKL = "Intel(R) Serial IO SPI Host Controller - A129"
iaLPSS2_SPI.DeviceDesc3_SKL = "Intel(R) Serial IO SPI Host Controller - A12A"
iaLPSS2_SPI.DeviceDesc4_SKL = "Intel(R) Serial IO SPI Host Controller - A2A9"
iaLPSS2_SPI.DeviceDesc5_SKL = "Intel(R) Serial IO SPI Host Controller - A2AA"
;-------------------iaLPSS2_SPI_TGL
iaLPSS2_SPI.DeviceDesc0_TGL = "Intel(R) Serial IO SPI Host Controller - A0AA"
iaLPSS2_SPI.DeviceDesc1_TGL = "Intel(R) Serial IO SPI Host Controller - A0AB"
iaLPSS2_SPI.DeviceDesc2_TGL = "Intel(R) Serial IO SPI Host Controller - A0FB"
iaLPSS2_SPI.DeviceDesc3_TGL = "Intel(R) Serial IO SPI Host Controller - A0FD"
iaLPSS2_SPI.DeviceDesc4_TGL = "Intel(R) Serial IO SPI Host Controller - A0FE"
iaLPSS2_SPI.DeviceDesc5_TGL = "Intel(R) Serial IO SPI Host Controller - A0DE"
iaLPSS2_SPI.DeviceDesc6_TGL = "Intel(R) Serial IO SPI Host Controller - A0DF"
iaLPSS2_SPI.DeviceDesc7_TGL = "Intel(R) Serial IO SPI Host Controller - 43AA"
iaLPSS2_SPI.DeviceDesc8_TGL = "Intel(R) Serial IO SPI Host Controller - 43AB"
iaLPSS2_SPI.DeviceDesc9_TGL = "Intel(R) Serial IO SPI Host Controller - 43FB"
iaLPSS2_SPI.SVCDESC = "Intel(R) Serial IO SPI Driver v2"
