
                MonitorMice for Windows NT 4.0
                        Release 3.10e
                        June 7, 2000

                     Elo TouchSystems, Inc.

MonitorMice for Windows NT contains a native, 32-bit driver
designed for Windows NT, setup program, uninstall utility,
and 32-bit control panel program, and DOS-based diagnostic
applications for Elo TouchSystems' touchscreens.

MonitorMice for Windows NT supports from 1 to 4 serial
touchmonitors connected to a single Windows NT 4.0
Workstation.

=======================================================
Supported Elo Touchscreen Controllers and Touchmonitors
=======================================================

   - SmartSet Serial Controllers: IntelliTouch(R) 2310,
     2300 and AccuTouch(R) 2210 and COACh

   - All Elo Entuitive brand touchmonitors

   -------------------------------------------------------
  | This driver does not support Elo PC-Bus controllers.  |
  |                                                       |
  | PC-Bus controllers require MonitorMouse 2.0 for       |
  | Windows NT available at www.elotouch.com.             |
   -------------------------------------------------------

=========================================
Installing MonitorMice for Windows NT 4.0
=========================================

Note: you must have administrator access rights on the Windows
NT 4.0 system to install MonitorMice for Windows NT 4.0. You
must also have adminstrator access rights to run the
touchscreen control panel and calibration applications.

1.  Shutdown Windows NT and turn off your computer.

2.  Install your Elo touchscreen hardware as described in the
    IntelliTouch or AccuTouch Product Manual, or the Quick Start
    poster.

3.  Start your computer.

4.  After Windows loads, click the Start button, and then click
    Run.

5.  Click the Browse button to locate the setup.exe program in
    the directory containing the driver install files. Click 
    Open, then OK to run setup.exe.

6.  Follow the directions on the screen to complete the Setup
    program.

7.  Restart your computer when prompted. The touchscreen
    calibration program will automatically run when Windows
    starts up. Touch each of the three targets as they appear
    on the screen. Click Yes when the cursor lines up correctly
    with your finger.

=================================
Changing the Touchscreen COM Port
=================================

If you selected the wrong COM port for the touchscreen during
installation of a single touchscreen configuration or want to
change these settings:

1. Choose Start/Settings/Control Panel and double-click
   the Elo Touchscreen object.

2. Select the correct COM port for the touchscreen
   controller. Click OK to close the touchscreen
   control panel.

3. Restart the computer when prompted.

Note: to change COM ports for multiple touchscreen
configurations, uninstall then reinstall the driver
as detailed below.

=======================
Uninstalling the Driver
=======================

1. Click the Start button, point to Settings, and then click
   Control Panel.

2. Double-click the Add/Remove Programs icon.

3. Select MonitorMice for Windows NT from the list of
   uninstallable programs on the Install/Uninstall tab.

4. Click the Add/Remove button then follow the directions on
   your screen.

5. Restart Windows NT when prompted to complete the uninstall
   process.

=============
Release Notes
=============

- To enable the "2-wire", no-handshaking mode, set the
  following DWORD registry key to 0 using regedit.exe:

   HKEY_LOCAL_MACHINE\System\CurrentControlSet\Services
      \Monmouse\TouchscreenXX\Parameters\HardwareHandShaking

  where "TouchscreenXX" is the registry section for the
  touchscreen for which the no-handshaking mode is to be
  enabled.

- Because serial communications services are not available
  until late in the Windows NT 4.0 startup process, the
  touchscreen will not begin to function for several seconds
  after the Windows NT logon dialog is displayed.

==========================================
Enhancements and Bug Fixes in This Release
==========================================

- Corrected a bug in the driver that caused the Enable and
  Disable IOCtl functions to fail.

==========
Known Bugs
==========

- The touchscreen control panel always displays "1" for the
  touchscreen COM port even if another COM port is actually
  in use. This bug does not affect the usage of this control
  to change the touchscreen COM port.

- It's easy to lose track of the touchscreen control panel if
  it is open on the Windows desktop, but underneath other
  windows. Relaunching the touchscreen control panel does
  not make the control panel visible. Instead, use Alt-Tab or
  the Taskbar to force the control panel to the top of the
  desktop.

- The Apply and Cancel buttons in the touchscreen control
  panel do not follow the accepted standard Windows conventions
  for functionality of these buttons in a control panel. The
  Apply button is not always available after modifying control
  panel options. The Cancel button doesn't cancel some settings
  that take effect immediately.

==============
Contacting Elo
==============

www.elotouch.com

e-mail: eloinfo@elotouch.com

Elo TouchSystems, Inc.
6500 Kaiser Drive
Fremont, CA 94555
USA
Phone: (800) 557-1458
       (510) 739-4999
Fax:   (510) 739-5353

Elo TouchSystems GmbH & Co. KG
Haidgraben 6
D-85521 Ottobrunn
Germany
Phone: +49 (0) 89/60822-0
Fax:   +49 (0) 89/60822-150

Elo TouchSystems, NV
Diestsesteenweg 692
B-3010 Kessel-Lo
Belgium
Phone: +32 (16) 35-2100
Fax:   +32 (16) 35-2101

Copyright (c) 2000 Elo TouchSystems, Inc.
All rights reserved.
