How to set printer IP address/DHCP , below are the steps to make it.

(1)Do the self test to check the currently IP address of the printer , the default should be : 192.168.1.251
(2)Connect LAN cable with printer to PC and set IP and Mask to Ethernet card of your PC(POS) , the IP should be the same section with printer , like IP : 192.168.1. X  ; Mask :255.255.255.0
(3)Type http://192.168.1.251 to open the printer configuration page with browser .
(4)Press Configure Interface on page left side to enter setting page. (Access info  User : admin ; no password needed)
(5)Change IP at “Fixed IP Address”or select DHCP and press “Save” button
(6)Press “Reboot” button to re-initial the new IP address/DCHP
(7)Do the self test to check the new IP address or DHCP configuration
